{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["sheet23-1"],"not_rendered":{"images":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"sheet23-1","index":0,"n_rows":45,"n_cols":32,"rows_kept":45,"merged":[[2,1,5,9],[2,10,2,21],[2,22,2,33],[3,22,3,24],[3,25,3,27],[3,28,3,30],[3,31,3,33],[4,22,4,24],[5,22,5,24],[5,25,5,27],[5,28,5,33],[6,13,6,19],[6,20,6,26],[6,27,6,33],[7,13,8,19],[7,20,8,26],[7,27,8,33],[9,13,9,19],[9,20,9,26],[9,27,9,33],[10,13,10,19],[10,20,10,26],[10,27,10,33],[12,13,12,19],[12,20,12,26],[12,27,12,33],[13,13,13,19],[13,20,13,26],[13,27,13,33],[14,13,14,19],[14,20,14,26],[14,27,14,33],[15,13,15,19],[15,20,15,26],[15,27,15,33],[16,13,16,19],[16,20,16,26],[16,27,16,33],[17,13,17,19],[17,20,17,26],[17,27,17,33],[18,13,18,19],[18,20,18,26],[18,27,18,33],[19,13,19,19],[19,20,19,26],[19,27,19,33],[21,13,21,19],[21,20,21,26],[21,27,21,33],[22,13,22,19],[22,20,22,26],[22,27,22,33],[23,13,23,19],[23,20,23,26],[23,27,23,33],[24,13,24,19],[24,20,24,26],[24,27,24,33],[25,13,25,19],[25,20,25,26],[25,27,25,33],[26,13,26,19],[26,20,26,26],[26,27,26,33],[27,13,27,19],[27,20,27,26],[27,27,27,33],[28,13,28,19],[28,20,28,26],[28,27,28,33],[29,13,29,19],[29,20,29,26],[29,27,29,33],[30,13,30,19],[30,20,30,26],[30,27,30,33],[31,13,31,19],[31,20,31,26],[31,27,31,33],[32,13,32,19],[32,20,32,26],[32,27,32,33],[33,13,33,19],[33,20,33,26],[33,27,33,33],[34,13,34,19],[34,20,34,26],[34,27,34,33],[35,13,35,19],[35,20,35,26],[35,27,35,33],[36,13,36,19],[36,20,36,26],[36,27,36,33],[37,13,37,19],[37,20,37,26],[37,27,37,33],[44,1,44,2],[44,3,44,9],[44,10,44,14],[44,15,44,17],[44,18,44,22],[44,23,44,25],[44,26,44,30],[44,31,44,33]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":10},"仪表数据表\nINSTRUMENT DATA SHEET                                                                                                  "]
[{"$nulls":10},"转子流量计",{"$nulls":11},"工程号\nENG. NO.",{"$nulls":5},"主项号\nPROJ.NO."]
[{"$nulls":10},"VARIABLE AREA FLOWMETER",{"$nulls":11},"图号\nDWG. NO."]
[{"$nulls":22},"设计阶段\nSTAGE"]
[null,"位号 TAG NO."]
[]
[]
[null,"P&ID号 P&ID NO."]
[null,"管道编号 LINE NO."]
[null,"操作条件 OPERATING CONDITIONS"]
[null,"工艺介质 PROCESS FLUID",{"$nulls":11},"乙酯、乙醇、水、醋酸\n"]
[null,"操作压力 OPER.PRESS. MPa(G)",{"$nulls":11},"0.3MPa"]
[null,"操作温度 OPER. TEMPER.℃",{"$nulls":11},"40"]
[null,"最大流量 MAX.FLOW ",{"$nulls":11},"6m³/h"]
[null,"正常流量 NOR.FLOW ",{"$nulls":11},"3m³/h"]
[null,"最小流量 MIN.FLOW ",{"$nulls":11},"0m³/h\n"]
[null,"操作密度 OPER.DENSITY",{"$nulls":11},"964Kg/m3/h"]
[null,"操作状态粘度 VISC.AT OPER. mPa.s"]
[null,"流量计规格 FLOWMETER SPECIFICATION"]
[null,"型号 MODEL"]
[null,"测量范围 MEAS.RANGE",{"$nulls":11},"0~8m3/h\n"]
[null,"口径 DIAMETER",{"$nulls":11},"DN32"]
[null,"精度 ACCURACY",{"$nulls":11},"±1.6%"]
[null,"测量管材质 MEAS.PIPE MATERIAL",{"$nulls":11},"316L"]
[null,"浮子材质 LINING MATERIAL",{"$nulls":11},"316L"]
[null,"工艺连接形式 PROCESS CONN.STYLE",{"$nulls":11},"法兰"]
[null,"输出信号 OUTPUT SIGNAL",{"$nulls":11},"4~20mA带HART"]
[null,"电源 POWER SUPPLY",{"$nulls":11},"24VDC\n"]
[null,"法兰标准及等级 FLANGE STD.& RATING",{"$nulls":11},"HG/T20592-2009 PN16"]
[null,"法兰尺寸及密封面 FLANGE SIZE & FACING",{"$nulls":11},"DN32 RF"]
[null,"螺纹规格 THREAD SIZE"]
[null,"电气接口尺寸 ELEC.CONN.SIZE",{"$nulls":11},"1/2NPT"]
[null,"防爆等级 EXPLOSION-PROOF CLASS",{"$nulls":11},"Exd IIBT4\n"]
[null,"防护等级 ENCLOSURE PROOF",{"$nulls":11},"IP66"]
[null,"制造厂 MANUFACTURER"]
[null,"数量 QUANTITY",{"$nulls":11},"3"]
[null,"备注 REMARKS",{"$nulls":11},"底进上出，线性刻度，带输出指示表：指针+数字,法兰间距245mm"]
[]
[]
[]
[]
[{"$nulls":14},"  "]
[null,"修 改\nREV.",null,"说    明\nDESCRIPTION",{"$nulls":6},"设  计\nDESD",{"$nulls":4},"日 期\nDATE",null,null,"校  核\nCHED",{"$nulls":4},"日 期\nDATE",null,null,"审   核\nAPPD",{"$nulls":4},"日 期\nDATE"]