{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"merged":[[0,0,0,8],[28,0,28,8]]}
[" 2024年索普股份年度消防器材采购清单"]
["序号","物料名称","规格型号","品牌","单位","数量","含税\n（单价）","含税\n（总价）","交货期"]
[1,"二氧化碳灭火器MT/2","MT/2手提式，2kg，执行标准：GB4351.2-2005。",null,"个",40]
[2,"手提式干粉灭火器FMZ4-ABC","FMZ4-ABC，4kg，执行标准：GB4351.1-2005。",null,"个",900]
[3,"推车式干粉灭火器35KG","35kg,执行标准:GB8109-2005,含配套推车。",null,"个",25]
[4,"推车式CO2灭火器24kg","24kg,执行标准:GB8109-2005,含配套推车。",null,"个",6]
[5,"水炮","固定式，水雾-直流两用，流量40L/S 射程60米，符合设计规范：GB50338-2003的要求。",null,"个",12]
[6,"室内消防栓","SN65，执行标准：GB3445-2018。",null,"个",35]
[7,"室外地上消防栓","SS100/65-1.6，执行标准：GB4452-2011。",null,"个",45]
[8,"灭火器箱","XMDF4-4（304不锈钢材质，壁厚1mm），用于4kg*4只，执行标准：GA139-2009。",null,"个",250]
[9,"室内消火栓箱","钢-铝合金65×24×80，铝合金门窗，箱体镀锌板材厚度1mm，执行标准：GB14561-2003。",null,"个",35]
[10,"室外消防水带箱","轿顶式，70×24×115铝合金门窗，箱体镀锌板材厚度1.2mm，执行标准：GB/T 14561-2019。",null,"个",200]
[11,"消防扳手","通用型，执行标准：GB4452-2011。",null,"个",20]
[12,"消防水带","有衬里10-65-25涤纶长丝-合成橡胶（含捆扎好的卡口接扣，接口处用铅丝捆扎二道 外部加接口保护套），水带以非黑色的有色线作为带身中心线，在端部附近中心线两侧应用不易脱落的油墨，清晰地印有：产品名称、规格型号、生产厂名、注册商标和生产日期，编织层织物层应编织均匀，表面整洁，无跳双经、断双经、跳纬及划伤。在设计工作压力下，不应发生渗漏和爆破,水带与消防接口连接处不应发生渗漏、爆破或滑脱。执行标准：GB6246-2011，长25米。",null,"个",500]
[13,"消防水枪","直流卡口，执行标准：GB8181-2005。",null,"个",20]
[14,"消火栓封盖","消火栓闷盖，用于消火栓65的接口，执行标准：GB4452-2011",null,"个",20]
[15,"泡沫管枪","（快口、卡口）QP4/0.7Z,混合比6%",null,"个",15]
[16,"消防水带","有衬里16-65-25涤纶长丝-合成橡胶（含捆扎好的快口接扣，接口处用铅丝捆扎二道 外部加接口保护套），水带以非黑色的有色线作为带身中心线，在端部附近中心线两侧应用不易脱落的油墨，清晰地印有：产品名称、规格型号、生产厂名、注册商标和生产日期，编织层织物层应编织均匀，表面整洁，无跳双经、断双经、跳纬及划伤。在设计工作压力下，不应发生渗漏和爆破,水带与消防接口连接处不应发生渗漏、爆破或滑脱。执行标准：GB6246-2011，长25米。",null,"个",110]
[17,"水带接扣","执行标准：GB12514.1-2005；GB12514.2-2006，Ф65卡口。",null,"个",22]
[18,"直流喷雾两用水枪"," DN65、卡口",null,"个",20]
[19,"  灭火毯（国产）","执行标准：GA1205-2014 规格：1.5米 X 1.5米，玻璃纤维材质",null,"块",500]
[20,"  防火布","1.0*1.0 m；厚度2mm执行标准：GA1205-2014玻璃纤维材质",null,"块",330]
[21,"  不锈钢灭火器箱","执行标准:GA139-2009，不锈钢材质，4Kg干粉灭火器，2只装",null,"个",110]
[22,"消防水带","有衬里16-150-30涤纶长丝-合成橡胶（含捆扎好的快口接扣，接口处用铅丝捆扎二道 外部加接口保护套）水带以非黑色的有色线作为带身中心线，在端部附近中心线两侧应用不易脱落的油墨，清晰地印有：产品名称、规格型号、生产厂名、注册商标和生产日期，编织层织物层应编织均匀，表面整洁，无跳双经、断双经、跳纬及划伤。在设计工作压力下，不应发生渗漏和爆破,水带与消防接口连接处不应发生渗漏、爆破或滑脱。执行标准：GB6246-2011，",null,"条",220]
[23,"泡沫发生器密封玻璃","直径136mm，厚度2mm, 一个圆加画十字",null,"个",80]
[24,"手提式磷酸酸盐干粉灭火器","MFZ/ABC5",null,"只",25]
[25,"推车式干粉灭火器50KG","50kg,MFTZ/ABC50，执行标准:GB8109-2005,含配套推车。",null,"个",6]
[26,"消防专用手套","执行标准：GA7-2004,14款",null,"付",10]
["备注：随货包装完好，标识清楚，提供相关3C认证、质保书或合格证等。交货期为收到计划后到货时间，建议一般器材收到供货计划后10天内到。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}