{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["报价表"],"read":"whole","date_system":"1900"}

{"sheet":"报价表","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"merged":[[0,0,0,13],[3,1,5,1],[3,13,9,13],[6,1,7,1],[8,1,9,1],[11,0,11,13],[12,0,12,1],[12,2,12,3],[12,5,12,6],[12,8,12,10],[12,11,12,12],[13,0,13,1],[13,2,13,3],[13,5,13,6],[13,8,13,10],[13,11,13,12],[14,0,14,1],[14,2,14,3],[14,5,14,6],[14,8,14,10],[14,11,14,12],[15,0,15,1],[15,2,15,3],[15,5,15,6],[15,8,15,10],[15,11,15,12],[16,0,16,1],[16,2,16,3],[16,5,16,6],[16,8,16,10],[16,11,16,12],[17,0,17,1],[17,2,17,3],[17,5,17,6],[17,8,17,10],[17,11,17,12],[18,0,18,1],[18,2,18,3],[18,5,18,6],[18,8,18,10],[18,11,18,12],[19,0,19,1],[19,2,19,3],[19,5,19,6],[19,8,19,10],[19,11,19,12],[20,0,22,13],[23,0,23,13]]}
["盘扣脚手架租赁报价表"]
["序号","物资名称","计算规格\n（不低于此规格）","投标钢管规格","计算规格\n尺寸型号(mm)","投标规格\n尺寸型号(mm)","钢材等级不低于此要求","暂估使用量（根）","暂估租赁时间（天）","参考        理论重量\n（kg/根）","投标           理论重量\n（kg/根）","含税租赁单价\n（见备注）\n（¥：元）","含税合计报价（¥：元）","备注"]
[1,"托座","Ф48×6.5×600",null,"A-ST-600",null,"Q235B",3594,60,"/","/",null,{"$f":"H3*L3*I3","v":{"v":0,"d":"0.00"}},"租赁单价为（      元/根/天）\n结算方式：暂估使用量X含税租赁单价X暂估使用天数"]
[2,"水平杆","Ф42×2.5×540",null,"B-SG-600",null,"Q235B",2385,60,{"v":2.3,"d":"2.30"},null,null,{"$f":"H4*K4*L4*I4","v":{"v":0,"d":"0.00"}},"租赁单价为（      元/吨/天）\n结算方式：暂估使用量X投标理论重量X含税租赁单价X暂估使用天数/1000"]
[3,null,"Ф42×2.5×840",null,"B-SG-900",null,"Q235B",1864,60,{"v":3.2,"d":"3.20"},null,null,{"v":0,"d":"0.00"}]
[4,null,"Ф42×2.5×1140",null,"B-SG-1200",null,"Q235B",11621,60,{"v":4.1,"d":"4.10"},null,null,{"v":0,"d":"0.00"}]
[5,"立杆","Ф48×3.2×500",null,"B-LG-500",null,"Q355",3536,60,2.95,null,null,{"v":0,"d":"0.00"}]
[6,null,"Ф48×3.2×2000",null,"B-LG-2000",null,"Q355",4060,60,{"v":9.9,"d":"9.90"},null,null,{"v":0,"d":"0.00"}]
[7,"竖向斜杆","Ф33×2.3×1710",null,"B-XG-900*1500",null,"Q195",440,60,{"v":4.1,"d":"4.10"},null,null,{"v":0,"d":"0.00"}]
[8,null,"Ф33×2.3×1859",null,"B-XG-1200*1500",null,"Q195",2500,60,{"v":4.4,"d":"4.40"},null,null,{"v":0,"d":"0.00"}]
[9,"运输费","/","/","运输车辆载重要求： 载重不低于10吨","/","/","暂估使用量 ：40车次","/","/","/","单车次费用\n（           元/车次）",{"v":0,"d":"0.00"},"结算方式：暂估使用车次X单车次费用"]
["盘扣脚手架赔偿费用表"]
["序号",null,"损坏类别",null,"单位","赔偿标准(元)",null,"序号","损坏类别",null,null,"单位",null,"赔偿标准(元)"]
[1,null,"盘扣立杆连接盘变形",null,"个",null,null,1,"包装架有物报废",null,null,"个"]
[2,null,"盘扣立杆端口变形",null,"个",null,null,2,"包装架丢失赔偿",null,null,"个"]
[3,null,"盘扣弯曲",null,"根",null,null,3,"盘扣顶、底托有物报废",null,null,"个"]
[4,null,"盘扣管内堵塞",null,"米",null,null,4,"盘扣顶、底托丢失赔偿",null,null,"个"]
[5,null,"盘扣横杆嵌板丢失",null,"个",null,null,5,"表面严重砂浆、涂油漆",null,null,"米"]
[6,null,"顶托底座变形损坏",null,"个",null,null,6,"盘扣有物报废",null,null,"米"]
[7,null,"顶托螺母丢失损坏",null,"个",null,null,7,"盘扣丢失赔偿",null,null,"米"]
["备注：\n1、以上报价都为含税报价，注明税率           %。\n2、按项目暂估使用数填报合计价格，汇总合计金额作为评标报价。\n3、赔偿费因占比例较小，未暂估数量，投标人只需报单价，实际发生时按实结算。\n4、入场钢管，抽检次数不固定，取平均数。抽检的质量问题租赁材料，按照百分比在结算时扣除。\n5、在归还后必须当天过数，归还清单上注明归还、损坏的详细数量。\n6、以上含税租赁单价，包含租赁材料、盘扣架的上力、下力费，包含租赁材料、顶托、盘扣架的清洗上油费用。\n7、我单位招标使用的盘扣种类规格为力学验算后的安全经济值，如投标托座、水平杆、立杆、竖向斜杆与我单位要求规格不一致，\n报价函中对标书的偏离项需注明，投标时注明规格、尺寸型号，按投标理论重量进行报价。"]
[]
[]
["租赁材料满足建筑施工承插型盘扣式钢管脚手架安全技术标准JGJ/T231-2021，JGT503-2016关于使用安全、质量尺寸偏差要求"]